ATNM Proposals Prioritisation – Benefits Scoring Criteria
	ScoreActive Travel Scheme Prioritisation – benefits scoring v.1


	Convenience
	Accessibility
	Safety
	Comfort
	Attractiveness
	Impact on other road users
	Impact on Health
	
	Score

	Potential to induce modal shift

	2
	· Route is direct for journeys for which it is expected to cater
· Route is essentially level
· Route contains few points of delay and/or avoids existing delays
	Provides significantly improved link -
· along identified desire line
· to key trip generator(s)
· between two existing links
· across existing severance

Proposal also readily accessible from all streets and premises
	Addresses significant recorded collision history (4 in 3 yrs, or 2 KSI in 3 yrs suggested)
	Significantly improves comfort (i.e. provides complete segregation from traffic with buffer, a well overlooked route, minimal traffic speeds etc.)
	Proposals significantly improve the environment for cycling /pedestrians in terms of aesthetics, noise, and quality of public space (i.e. through enhancement of Green Infrastructure and improvements in air quality)
	Scheme provides significant additional benefits to other road users. 
	Route connects to area ranked <250 in the Health Indicator of the WIMD.
	
	5
	Likely to result in significant modal shift from private car to pedal cycle/foot either as a result of the physical connection or route being within an area benefitting from an on-going behaviour change programme



	1
	· Route reasonably direct for journeys for which it is expected to cater
· Route includes only moderate gradients
· Route contains some points of delay and/or reduces existing delays
	Provides improved links -
· along identified desire line
· to key trip generator(s)
· between two existing links
· across existing severance

May also improve slightly accessibility to other streets and premises
	Addresses lesser recorded collision history, or location understood to have a collision history which is not fully recorded


	Improves comfort (i.e. provides some segregation from traffic, traffic speeds below 20mph without segregation, personal safety improvements such as CCTV and lighting etc.)
	Proposals slightly improve the environment for cycling/walking in terms of aesthetics, noise, and quality of public space (i.e. through enhancement of Green Infrastructure and improvements in air quality)
	Provides some additional benefit to other road users on balance (as a toucan might for pedestrians)
	Route connects to area ranked between 251 and 500 in the Health Indicator of the WIMD.
	
	3
	May increase numbers of cyclists/pedestrians but unlikely to result in significant modal shift from private cars either as a result of physical works or the route connecting to an area benefitting from a behaviour change programme 



	0
	· Proposals do not offer greater convenience than existing situation
	Proposals do not improve accessibility
	No expected impact on collisions
	No expected improvement in terms of comfort
	Proposals have little or no benefit on quality of environment for cycling/walking in terms of aesthetics, noise, and quality of public space
	No significant expected impact for other road users
	Route connects to area ranked >500 in the Health Indicator of the WIMD.
	
	0
	Little or no modal shift expected and scheme not linked to behaviour change programme



	-1
	· Proposal requires less direct route than existing
· Route introduces points of delay
	Unlikely to occur in practice
	Proposals may result in additional collisions
	May reduce level of comfort for cyclists/pedestrians




	Proposals degrade quality of environment for cycling/walking in terms of aesthetics, noise, and quality of public space
	Some significant negative impact expected for other road users (i.e. loss of residential parking, some additional congestion
	Unlikely to occur in practice
	
	-1
	Unlikely to occur in practice

	-2
	Unlikely to occur in practice
	Unlikely to occur in practice
	Unlikely to occur in practice
	Unlikely to occur in practice
	Unlikely to occur in practice
	Very significant negative impact expected for other road users (i.e. serious congestion, especially for PT, loss of parking in retail areas, restrictions on loading
	Unlikely to occur in practice
	
	-2
	Unlikely to occur in practice



